SECTION 26 5213

PHOTOLUMINESCENT EXIT SIGNS

This section includes editing notes to assist the user in editing the section to suit project requirements. These notes are included as hidden text, and can be revealed or hidden by one of the following methods:

Microsoft Word 2007: Click the OFFICE button, select WORD OPTIONS, select DISPLAY, then select or deselect the HIDDEN TEXT option.

Microsoft Word (earlier versions): From the pull-down menus select TOOLS, then OPTIONS. Under the tab labeled VIEW, select or deselect the HIDDEN TEXT option.

Corel WordPerfect: From the pull-down menus select VIEW, then select or deselect the HIDDEN TEXT option.

This master specification section has been prepared by EverGlow NA, Inc. for use in the preparation of a project specification section covering photoluminescent exit signs.

EverGlow NA, Inc. also offers photoluminescent (luminous) egress path markings including ADA and other signs, exit and evacuation maps, and stair nosings, stair, handrail, obstacle, and directional markers; refer to specification Section 10 1443 - Photoluminescent (Luminous) Egress Path Markings.

The following should be noted in using this specification:

Hypertext links to specific websites are included after manufacturer names and names of organizations whose standards are referenced within the text, to assist in product selection and further research. Hypertext links are contained in parenthesis and shown in blue, e.g.:

(www.nfpa.org)

Optional text requiring a selection by the user is enclosed within brackets, e.g.: "Section [09 0000.] [_____.]"

Items requiring user input are enclosed within brackets, e.g.: "Section [_____ - ________]."

Optional paragraphs are separated by an "OR" statement, e.g.:

**** OR ****

For assistance on the use of the products in this section, contact EverGlow NA, Inc. by calling toll-free 866-744-4706, by email at info@everglow.us, or visit their website at www.everglow.us.

PART 1	GENERAL

1.1	SUMMARY

A.	Section Includes:

1.	Photoluminescent [ceiling] [over-door] [floor level] [____] exit signs.

Coordinate the following paragraphs with other sections in the project manual.

B.	Related Sections:

1.	Division 01: Administrative, procedural, and temporary work requirements.

2.	Section 10 1443 - Photoluminescent (Luminous) Egress Path Markings.

3.	Section [26 5200] [16 520]: Emergency Lighting and Exit Signs.

1.2	REFERENCES

A.	National Fire Protection Association (NFPA) (www.nfpa.org) 101 - Life Safety Code.

B.	Underwriters Laboratories, Inc. (UL) (www.ul.com) - 924 - Standard for Emergency Lighting and Power Equipment.

1.3	QUALITY ASSURANCE

Edit the following to suit project requirements.

A.	Provide exit signs in accordance with [NFPA 101.] [Building Code.] [Fire Code.]

1.4	SUBMITTALS

Limiting submittals to only those actually required helps to minimize liability arising from the review of submittals. Minimize submittals on smaller, less complex projects.

Include the following for submission of shop drawings, product data, and samples for the Architect's review.

A.	Submittals for Review:

1.	Shop Drawings: Indicate exit sign locations, mounting heights, and attachments.

2.	Product Data: Include product description, materials, finishes, and performance characteristics.

3.	Samples: One full size exit sign. [Sample will be returned for installation on project.]

1.5	DELIVERY, STORAGE AND HANDLING

A.	Store exit signs in a dry location until installed.

1.6	WARRANTIES

A.	Provide manufacturer's limited warranty:

1.	Signs and markings installed in interior locations: 25 years.

2.	Signs and markings installed in exterior locations: 3 years.

PART 2	PRODUCTS

2.1	MANUFACTURERS

A.	Contract Documents are based on products by EverGlow NA, Inc. (www.everglow.us)

Edit the following to indicate whether or not substitutions will be permitted for the products in this section.

B.	Substitutions: [Under provisions of Division 01.] [Not permitted.]

2.2	MANUFACTURED UNITS

A.	Photoluminescent Exit Signs:

1.	Description:

a.	Sign face, frames, and mounting brackets: Aluminum, minimum 60 percent post-
consumer recycled content.

b.	Sign face: Aluminum sheet with photoluminescent markings.

c.	Absorb and store energy from ambient light, not requiring external power supply, lamps, LED's or batteries.

d.	Non-toxic, non-radioactive.

e.	High-visibility illumination.

f.	Free from vinyl and polyvinyl chloride compounds.

g.	Manufactured using low-VOC inks and coatings.

h.	UL approved for use in interior locations with fluorescent lighting.

i.	Tested and listed to UL 924.

2.	Background color of sign face: [Green.] [Red.] [Black.]

3.	Frame ;type: [Aluminum framed, [standard profile], [low profile] type.] [Unframed.] [As indicated in Schedule at end of Section.] [As indicated on Drawings.]

4.	Frame finish: [Clear anodized.] [Black.]

5.	Sign type: [One sided.] [Two sided.] [As indicated in Schedule at end of Section.] [As indicated on Drawings.]

6.	Mounting type: [Wall.] [Ceiling.] [Projected.] [As indicated in Schedule at end of Section.] [As indicated on Drawings.]

Include the following when mounting brackets are required.

7.	Mounting brackets: Manufacturer's standard for frame system, aluminum, [clear anodized] [black] finish.

8.	Directional indicators: Two self-adhering chevron profile indicators per sign, for field application.

9.	Sign size:

a.	Sign face: Approximately 8.6 inches high x 13.7 inches wide.

b.	Sign with frame: Approximately 9.3 inches high x 14.4 inches wide.

10.	Lettering: "EXIT" in 7 inch high letters with 7/8 inch stroke.

11.	Performance characteristics:

a.	Meet NFPA 101, Building Code, and Fire Code requirements for internally illuminated exit signs.

b.	Visible at 75 feet in total darkness.

c.	Tested by ETL; listed to UL 924.

d.	Service life: Minimum 25 years for interior installations.

2.3	ACCESSORIES

A.	Fasteners: Stainless or corrosion-resistant; type best suited to application.

PART 3	EXECUTION

3.1	INSTALLATION

A.	Install signs in accordance with [NFPA 101,] [Building Code,] [Fire Code,] manufacturer's instructions, and approved Shop Drawings.

Edit the following to suit project requirements.

B.	Locate signs to conform to [NFPA 101.] [Building Code.] [Fire Code.]

C.	Set signs plumb, level, and rigid.

D.	Attach signs to supporting construction.

E.	Attach directional arrow chevrons to sign faces to suit project requirements.

3.2	FIELD QUALITY CONTROL

A.	With room light fixtures illuminated, measure amount of illumination on face of each exit sign using handheld light meter.

B.	Ensure that each location has minimum of 5 foot-candles of illumination.

3.3	EXIT SIGN SCHEDULE

Include the following for a schedule listing the products in this section; edit to suit project requirements. Coordinate with Part 2 - Products and with drawing designations. The following may assist in developing a schedule.

SIGN DESIGNATION	SIGN TYPE	MOUNTING TYPE	MOUNTING HEIGHT
ES-1	Double sided	Projected	Ceiling or Wall
ES-2	Single sided	Projected	Ceiling or Wall
ES-3	Single sided	Wall	Over door or Floor level

END OF SECTION